               EPSON TM Flash LOGO Setup Utility for NVRAM Version 2.60Eb
               Release Note

                                  SEIKO EPSON CORPORATION
                                                                May 30, 2008
1. TM Flash Logo Utility Introduction
  The TMFlogo Utility is a utility for uploading image data to EPSON devices 
  (TM series printers or Line Display DM-D500) that have NVRAM bitmap image.
  You can use this utility to load external images, register NV bit images, 
  print or display the images, and store the registered image to files.

2. Supported Devices

   If the printer name includes "M", which means that the printer is either
   Simplified Chinese or Traditional Chinese.

    TM-H5000II    TM-H5000IIE    TM-H5000IIU    TM-H5000IIP
    TM-H5000IIM   TM-H5000IIME   TM-H5000IIMU   TM-H5000IIPM
    TM-H5200      TM-H5200E      TM-H5200U      TM-H5200P
    TM-H6000II    TM-H6000IIE    TM-H6000IIU    TM-H6000IIP
    TM-H6000IIM   TM-H6000IIME   TM-H6000IIMU   TM-H6000IIPM
    TM-H6000III   TM-H6000IIIE   TM-H6000IIIU   TM-H6000IIIP
    TM-H6000IIIM  TM-H6000IIIME  TM-H6000IIIMU  TM-H6000IIIPM
    TM-J2000      TM-J2000E      TM-J2000U      TM-J2000P
    TM-J2000M     TM-J2000ME     TM-J2000MU     TM-J2000PM
    TM-J2100      TM-J2100E      TM-J2100U      TM-J2100P
    TM-J2100M     TM-J2100ME     TM-J2100MU     TM-J2100PM
    TM-J7000      TM-J7000E      TM-J7000U      TM-J7000P
    TM-J7100      TM-J7100E      TM-J7100U      TM-J7100P
    TM-J7500      TM-J7500E      TM-J7500U      TM-J7500P
    TM-J7600      TM-J7600E      TM-J7600U      TM-J7600P
    TM-J9000      TM-J9000E      TM-J9000U      TM-J9000P
    TM-J9100      TM-J9100E      TM-J9100U      TM-J9100P
    TM-L90        TM-L90E        TM-L90U        TM-L90P
    TM-L90M       TM-L90ME       TM-L90MU       TM-L90PM
    TM-P60        TM-P60W
    TM-P60PEELER  TM-P60PEELERW
    TM-T70        TM-T70E        TM-T70U        TM-T70P
    TM-T88III     TM-T88IIIE     TM-T88IIIU     TM-T88IIIP
    TM-T88IIIM    TM-T88IIIME    TM-T88IIIMU    TM-T88IIIPM
    TM-T88IV      TM-T88IVE      TM-T88IVU      TM-T88IVP
    TM-T88IVM     TM-T88IVME     TM-T88IVMU     TM-T88IVPM
    TM-T88IIIX
    TM-T88IIIXM
    TM-T90        TM-T90E        TM-T90U        TM-T90P
    TM-T90M       TM-T90ME       TM-T90MU       TM-T90PM
    TM-U220A      TM-U220AE      TM-U220AU      TM-U220AP
    TM-U220AM     TM-U220AME     TM-U220AMU     TM-U220APM
    TM-U220AM_BM  TM-U220AM_BME  TM-U220AM_BMU  TM-U220APM_BM
    TM-U220B      TM-U220BE      TM-U220BU      TM-U220BP
    TM-U220BM     TM-U220BME     TM-U220BMU     TM-U220BPM
    TM-U220BM_BM  TM-U220BM_BME  TM-U220BM_BMU  TM-U220BPM_BM
    TM-U220D      TM-U220DE      TM-U220DU      TM-U220DP
    TM-U220DM     TM-U220DME     TM-U220DMU     TM-U220DPM
    TM-U220DM_BM  TM-U220DM_DME  TM-U220DM_DMU  TM-U220DPM_BM
    TM-U675       TM-U675E       TM-U675U       TM-U675P
    TM-U675M      TM-U675ME      TM-U675MU      TM-U675PM
    BA-T500       BA-T500E       BA-T500U       BA-T500P
    EU-T400(*1)   EU-T400P(*1)   EU-T400U(*1)
    DM-D500
    
    *1 When you use the EU-T400 series, please select the
       "EU-T400", "EU-T400P" and "EU-T400U".

3. Other Considerations
  * EPSON OPOS ADK is confirmed its operations under the following OS environment.
    Windows 2000 professional Service Pack4
    Windows XP professional Service Pack2
    Windows Vista Ultimate/Business/Enterprise 
    
  * Manuals(Documentation files)
    Although the version number in the enclosed manuals is 2.60Ea, 
    these documents are also applicable to version 2.60Eb.

